[ALT-F] Particionado de disco duro desde ALT-F

ALT-F es un firmware que se puede instalar en el DNS323 y permite utilizar discos duros de más de 2 TB, al poder manejar tablas de particiones GPT.

Montamos el disco en el NAS y lo preparamos con el menú Disk → Wizard. En este caso se trata de un disco de 3 TB.

Damos a Abracadabra y el disco queda preparado para su uso.

Vamos ahora a analizar cómo han quedado las particiones en el mismo. Para ello usaré gdisk. Me conecto con una sesión ssh

ssh root@ip_NAS

Entrando con la misma contraseña que en el entorno gráfico web del firmware.

Para ver las particiones ejecutamos

gdisk /dev/sda

lo que nos muestra

[root@bkp]# gdisk /dev/sda
GPT fdisk (gdisk) version 1.0.1
Partition table scan:
MBR: protective
BSD: not present
APM: not present
GPT: present
Found valid GPT with protective MBR; using GPT.
Command (? for help):

Las opciones de este comando son

Command (? for help): ?
b	back up GPT data to a file
c	change a partition's name
d	delete a partition
i	show detailed information on a partition
l	list known partition types
n	add a new partition
o	create a new empty GUID partition table (GPT)
p	print the partition table
q	quit without saving changes
r	recovery and transformation options (experts only)
s	sort partitions
t	change a partition's type code
v	verify disk
w	write table to disk and exit
x	extra functionality (experts only)
?	print this menu

Command (? for help): p
Disk /dev/sda: 5860533168 sectors, 2.7 TiB
Logical sector size: 512 bytes
Disk identifier (GUID): D56AB725-99E4-4299-B299-D20B9A6C56A1
Partition table holds up to 128 entries
First usable sector is 34, last usable sector is 5860533134
Partitions will be aligned on 64-sector boundaries
Total free space is 30 sectors (15.0 KiB)
Number Start (sector) End (sector) Size Code Name
1 64 1429567 698.0 MiB 8200
2 1429568 5860533134 2.7 TiB 8300

Aquí podemos observar que se han creado dos particiones: una de intercambio swap de 698 MiB y otra linux de 2.7 TiB. Para más detalle:

Command (? for help): i
Partition number (1-2): 1
Partition GUID code: 0657FD6D-A4AB-43C4-84E5-0933C84B4F4F (Linux swap)
Partition unique GUID: D4083559-0F86-45A0-9599-52E8CC52F0D3
First sector: 64 (at 32.0 KiB)
Last sector: 1429567 (at 698.0 MiB)
Partition size: 1429504 sectors (698.0 MiB)
Attribute flags: 0000000000000000
Partition name: ''
Command (? for help): i
Partition number (1-2): 2
Partition GUID code: 0FC63DAF-8483-4772-8E79-3D69D8477DE4 (Linux filesystem)
Partition unique GUID: 04B463DE-59C8-4D37-88F8-6DE62601DDED
First sector: 1429568 (at 698.0 MiB)
Last sector: 5860533134 (at 2.7 TiB)
Partition size: 5859103567 sectors (2.7 TiB)
Attribute flags: 0000000000000000
Partition name: ''

que desde el entorno gráfico:

Ahora ya podemos comenzar a crear carpetas en la partición linux y luego darlas a compartir en smb .